==== EAS_audio_file_descriptor

Defined by ANSI/SCTE in <<SCTE-18>>.
Must be in a Cable Emergency Alert Table (table id 0xD8).

[source,xml]
----
<EAS_audio_file_descriptor>
  <!-- One entry per audio file -->
  <file audio_format="uint7, required"
        file_name="string, optional"
        audio_source="uint8, required"
        program_number="uint16, optional"
        carousel_id="uint32, optional"
        application_id="uint16, optional"
        download_id="uint32, optional"
        module_id="uint32, optional"/>
</EAS_audio_file_descriptor>
----
