==== CP_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<CP_descriptor CP_system_id="uint16, required" CP_PID="uint13, required">
  <private_data>
    Hexadecimal content
  </private_data>
</CP_descriptor>
----
