==== DTS_UHD_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<DTS_UHD_descriptor
    DecoderProfileCode="uint6, required"
    FrameDurationCode="uint2, required"
    MaxPayloadCode="uint2, required"
    StreamIndex="uint3, required">

  <codec_selector>
    Hexadecimal Content
  </codec_selector>

</DTS_UHD_descriptor>
----
