==== CA_identifier_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<CA_identifier_descriptor>
  <!-- One per CAS -->
  <CA_system_id value="uint16, required"/>
</CA_identifier_descriptor>
----
