==== splice_audio_descriptor

Defined by ANSI/SCTE in <<SCTE-35>>.
Must be in a Splice Information Table (table id 0xFC).

[source,xml]
----
<splice_audio_descriptor identifier="uint32, default=0x43554549">
  <!-- One per audio stream -->
  <audio component_tag="uint8, required"
         ISO_code="char3, required"
         Bit_Stream_Mode="uint3, required"
         Num_Channels="uint4, required"
         Full_Srvc_Audio="bool, required"/>
</splice_audio_descriptor>
----
