==== DTS_neural_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<DTS_neural_descriptor config_id="uint8, required">
  <additional_info>
    Hexadecimal content
  </additional_info>
</DTS_neural_descriptor>
----
