==== SSU_uri_descriptor

Defined by DVB in <<ETSI-102-006>>.
Must be in a UNT (table id 0x4B).

[source,xml]
----
<SSU_uri_descriptor
    max_holdoff_time="uint8, required"
    min_polling_interval="uint8, required"
    uri="string, required"/>
----

Warning: As defined in <<ETSI-102-006>>,
`max_holdoff_time` is a number of minutes and `min_polling_interval` is a number of hours.
