==== Related Content Table (RCT)

Defined by DVB in <<ETSI-102-323>>.

[source,xml]
----
<RCT version="uint5, default=0"
     current="bool, default=true"
     service_id="uint16, required"
     year_offset="uint16, required">

  <!-- One per link -->
  <link link_type="uint4, required"
        how_related_classification_scheme_id="uint6, required"
        term_id="uint12, required"
        group_id="uint4, required"
        precedence="uint4, required"
        media_uri="string, required when link_type == 0 or 2"
        default_icon_flag="bool, required"
        icon_id="uint3, required">

    <!-- If link_type == 1 or 2 -->
    <dvb_binary_locator
        identifier_type="uint2, required"
        scheduled_time_reliability="bool, required"
        inline_service="bool, required"
        start_date="uint9, required"
        dvb_service_triplet_id="uint10, required when inline_service == false"
        transport_stream_id="uint16, required when inline_service == true"
        original_network_id="uint16, required when inline_service == true"
        service_id="uint16, required when inline_service == true"
        start_time="uint16, required"
        duration="uint16, required"
        event_id="uint16, required when identifier_type == 1"
        TVA_id="uint16, required when identifier_type == 2 or 3"
        component_tag="uint8, required when identifier_type == 3"
        early_start_window="uint3, required when identifier_type == 0 and
                                   scheduled_time_reliability == true"
        late_end_window="uint5, required when identifier_type == 0 and
                                scheduled_time_reliability == true"/>

    <!-- One per text -->
    <promotional_text language_code="char3, required" text="string, required"/>

    <DESCRIPTOR_LIST>

  </link>

  <DESCRIPTOR_LIST>

</RCT>
----
