==== protection_message_descriptor

Defined by DVB in <<ETSI-102-809>>.

[source,xml]
----
<protection_message_descriptor>
  <!-- One per component, up to 15 components -->
  <component tag="uint8, required"/>
</protection_message_descriptor>
----
