==== EAS_inband_details_channel_descriptor

Defined by ANSI/SCTE in <<SCTE-18>>.
Must be in a Cable Emergency Alert Table (table id 0xD8).

[source,xml]
----
<EAS_inband_details_channel_descriptor
    details_RF_channel="uint8, required"
    details_program_number="uint16, required"/>
----
