==== DTS_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<DTS_descriptor
    sample_rate_code="uint4, required"
    bit_rate_code="uint6, required"
    nblks="uint7, 0x05 to 0x1F, required"
    fsize="uint14, 0x005F to 0x2000, required"
    surround_mode="uint6, required"
    lfe="bool, default=false"
    extended_surround="uint2, default=0">
  <additional_info>
    Hexadecimal content
  </additional_info>
</DTS_descriptor>
----
