==== ISDB_connected_transmission_descriptor

Defined by ARIB in <<ARIB-B10J>>.

[source,xml]
----
<ISDB_connected_transmission_descriptor
   connected_transmission_group_id="uint16, required"
   segment_type="uint2, required"
   modulation_type_A="uint2, required"
   modulation_type_B="uint2, required"
   modulation_type_C="uint2, required">

   <addtional_connected_transmission_info>
     Hexadecimal data
   </addtional_connected_transmission_info>

</ISDB_connected_transmission_descriptor>
----
