==== IPMAC_stream_location_descriptor

Defined by DVB in <<ETSI-301-192>>.
Must be in an INT (table id 0x4C).

[source,xml]
----
<IPMAC_stream_location_descriptor
    network_id="uint16, required"
    original_network_id="uint16, required"
    transport_stream_id="uint16, required"
    service_id="uint16, required"
    component_tag="uint8, required"/>
----
