==== Event Information Table (EIT)

Defined by ATSC in <<ATSC-A65>>.

To avoid conflicts with the DVB version of an EIT, the XML structure is named `<ATSC_EIT>`.
The tag `<EIT>` designates a DVB EIT.

[source,xml]
----
<ATSC_EIT version="uint5, default=0"
          source_id="uint16, required"
          protocol_version="uint8, default=0">

  <!-- One per event -->
  <event event_id="uint16, required"
         start_time="YYYY-MM-DD hh:mm:ss, required"
         ETM_location="uint2, required"
         length_in_seconds="uint20, required">

    <!-- Optional ATSC multiple_string_structure() containing one or more strings -->
    <title_text>
      <string language="char3, required" text="string, required"/>
    </title_text>

    <!-- Event descriptors loop -->
    <DESCRIPTOR_LIST>

  </event>

</ATSC_EIT>
----
