==== HEVC_operation_point_descriptor

Defined by MPEG in <<ISO-13818-1>>.

[source,xml]
----
<HEVC_operation_point_descriptor>

  <profile_tier_level_info>
    Hexadecimal Content
  </profile_tier_level_info>

  <operation_point
      target_ols="uint8, required"
      constant_frame_rate_info_idc="uint2, required"
      applicable_temporal_id="uint3, required"
      frame_rate_indicator="uint12, default=0"
      avg_bit_rate="uint24, default=0"
      max_bit_rate="uint24, default=0">
    <ES
        prepend_dependencies="bool, required"
        ES_reference="uint6, required"/>
    <ESinOP
        necessary_layer="bool, required"
        output_layer="bool, required"
        ptl_ref_idx="uint6, required"/>
  </operation_point>

</HEVC_operation_point_descriptor>
----
