# /etc/asterisk/zapata.conf:
# Digium/Clone T100P EXAMPLE:
# Here is an example of a configuration where an T100P single T1 card is used 
# for connecting a single T1 PRI circuit with 23 voice channels

[channels]
group=1
language=en
signalling=pri_net
usecallerid=yes
callerid=asreceived
callprogress=no
busydetect=no
context=default
echocancel=64
echocancelwhenbridged=yes
rxgain=1.0
txgain=1.0
channel => 1-23

# FOR A RBS WinkStart T1 YOU WOULD USE SOMETHING LIKE THIS:
# group=1
# language=en
# signalling=em_w
# usecallerid=yes
# callerid=asreceived
# context=default
# echocancel=64
# echocancelwhenbridged=yes
# rxgain=1.0
# txgain=1.0
# channel => 1-24
# 
# FOR AN ANALOG T1 ChannelBank YOU WOULD USE SOMETHING LIKE THIS:
# group=4
# language=en
# signalling=fxo_ks
# usecallerid=yes
# callerid=asreceived
# context=default
# echocancel=64
# echocancelwhenbridged=no
# rxgain=-1.0
# txgain=-1.0
# channel => 1-24

