# /etc/zaptel.conf:
# Digium/Clone X100P EXAMPLE:
# Here is an example of a configuration where an X100P single FXO card is used 
# for zaptel timing and not used for calling:
# 
# NOTE: you can get an X100P on ebay for $10-30 that will work with Asterisk

loadzone=us
defaultzone=us
fxsks=1
