==== ISDB_wired_multicarrier_transmission_descriptor

Defined by JCTEA in <<JCTEA-003>>.

This descriptor is also known under the following names:

[.compact-list]
* wired_multicarrier_transmission_distribution_system_descriptor (ARIB STD-B10)
* channel_bonding_cable_delivery_system_descriptor (JCTEA STD-003)

[source,xml]
----
<ISDB_wired_multicarrier_transmission_descriptor>

  <!-- One per carrier -->
  <carrier
      frequency="uint, frequency in Hz, required"
      frame_type="uint4, required"
      FEC_outer="uint4, required"
      modulation="uint8, required"
      symbol_rate="uint, in symbols/second, required"
      FEC_inner="uint4, default=15"
      group_id="uint8, required"/>

</ISDB_wired_multicarrier_transmission_descriptor>
----
