Ada Reference Manual (Ada 2022) — Legal Information

# 13.5.2 Storage Place Attributes

#### Static Semantics

1
For a component C of a composite, non-array object R, the storage place attributes are defined:
2/2
R.C'Position
If the nondefault bit ordering applies to the composite type, and if a component_clause specifies the placement of C, denotes the value given for the position of the component_clause; otherwise, denotes the same value as R.C'Address – R'Address. The value of this attribute is of the type universal_integer.
3/2
R.C'First_Bit
If the nondefault bit ordering applies to the composite type, and if a component_clause specifies the placement of C, denotes the value given for the first_bit of the component_clause; otherwise, denotes the offset, from the start of the first of the storage elements occupied by C, of the first bit occupied by C. This offset is measured in bits. The first bit of a storage element is numbered zero. The value of this attribute is of the type universal_integer.
4/2
R.C'Last_Bit
If the nondefault bit ordering applies to the composite type, and if a component_clause specifies the placement of C, denotes the value given for the last_bit of the component_clause; otherwise, denotes the offset, from the start of the first of the storage elements occupied by C, of the last bit occupied by C. This offset is measured in bits. The value of this attribute is of the type universal_integer.

#### Implementation Advice

5
If a component is represented using some form of pointer (such as an offset) to the actual data of the component, and this data is contiguous with the rest of the object, then the storage place attributes should reflect the place of the actual data, not the pointer. If a component is allocated discontiguously from the rest of the object, then a warning should be generated upon reference to one of its storage place attributes.

Ada 2005 and 2012 Editions sponsored in part by Ada-Europe