==== SSU_event_name_descriptor

Defined by DVB in <<ETSI-102-006>>.
Must be in a UNT (table id 0x4B).

[source,xml]
----
<SSU_event_name_descriptor ISO_639_language_code="char3, required"
  <name>String</name>
  <text>String</text>
</SSU_event_name_descriptor>
----
