==== service_move_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<service_move_descriptor
    new_original_network_id="uint16, required"
    new_transport_stream_id="uint16, required"
    new_service_id="uint16, required"/>
----
