==== multiplex_buffer_utilization_descriptor

Defined by MPEG in <<ISO-13818-1>>.

The two attributes must be both present or both absent.

[source,xml]
----
<multiplex_buffer_utilization_descriptor
    LTW_offset_lower_bound="uint15, optional"
    LTW_offset_upper_bound="uint15, optional"/>
----
