==== deferred_association_tags_descriptor

Defined by MPEG in <<ISO-13818-6>>.

[source,xml]
----
<deferred_association_tags_descriptor
    transport_stream_id="uint16, required"
    program_number="uint16, required">
  <!-- One per association tag -->
  <association tag="uint16, required"/>
  <private_data>
    Hexadecimal content
  </private_data>
</deferred_association_tags_descriptor>
----
