==== application_storage_descriptor

Defined by DVB in <<ETSI-102-809>>.
Must be in an AIT (table id 0x74).

[source,xml]
----
<application_storage_descriptor
    storage_property="uint8, required"
    not_launchable_from_broadcast="bool, required"
    launchable_completely_from_cache="bool, required"
    is_launchable_with_older_version="bool, required"
    version="uint31, required"
    priority="uint8, required"/>
----
