==== dvb_html_application_descriptor

Defined by DVB in <<ETSI-101-812>>.
Must be in an AIT (table id 0x74).

[source,xml]
----
<dvb_html_application_descriptor parameter="string, optional">
  <!-- One per application id: -->
  <application id="uint16, required"/>
</dvb_html_application_descriptor>
----
