==== local_time_offset_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<local_time_offset_descriptor>
  <!-- One per region -->
  <region country_code="char3, required"
          country_region_id="uint6, required"
          local_time_offset="int, required"
          time_of_change="YYYY-MM-DD hh:mm:ss, required"
          next_time_offset="int, required"/>
  <!-- local_time_offset and next_time_offset: -->
  <!-- -780 to +780 minutes (-13 to +13 hours) -->
</local_time_offset_descriptor>
----
