==== m4mux_timing_descriptor

Defined by MPEG in <<ISO-13818-1>>.

[source,xml]
----
<m4mux_timing_descriptor
    FCR_ES_ID="uint16, required"
    FCRResolution="uint32, required"
    FCRLength="uint8, required"
    FmxRateLength="uint8, required"/>
----
